Designed for little millet, fox tail millet, polishing of Finger millet and useful in breaking pigeon pea

In principle paddy can be dehusker but not yet experimented.

Operates on 1phase current, 2hp and portable.

 

